##
Time integration using the odefile

Time integration (= simulation) of the dynamical system can be done on the command line as in the following example:

    OPTIONS=[];
    hls = MyML;
    [t,y] = ode45(hls{2},[0 1000],[0 0],OPTIONS,30,10);
    x0 = y(end,:)';

In this example the system MyML is integrated over the interval starting with the input vector and with parameters in that order. The integration is performed with the integration routine ode45 with the defaults (OPTIONS=[]) in MATLAB. The output vector is placed in x0. More details are given in Chapter 5.